{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["PosstionStringSheet","污染物超标报表","Sheet1"],"not_rendered":{"images":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PosstionStringSheet","index":0,"n_rows":1,"n_cols":1,"rows_kept":1,"hidden":true,"flags":["formulas_cached_only"]}
["污染物超标报表=0|1,1,2,8;1|3,1,189,8;&"]

{"sheet":"污染物超标报表","index":1,"n_rows":189,"n_cols":9,"rows_kept":189,"merged":[[0,0,0,8],[1,0,1,8]],"flags":["formulas_cached_only"]}
["污染物超标报表"]
["关注程度：国控.省控.市控  监控点类型：废水.废气  监测时间：2021-03-01至2021-03-31"]
["企业名称","监控点名称","超标污染物","报警值","报警开始时间","报警结束时间","超标上下限","超标倍数","超标说明"]
["安徽马钢表面技术股份有限公司","废水排口","化学需氧量(COD)",84.7,"2021-03-05 21:00:00","2021-03-05 22:00:00","0~80",0.0588]
["安徽马钢表面技术股份有限公司","废水排口","化学需氧量(COD)",169,"2021-03-06 23:00:00","2021-03-07 03:00:00","0~80",1.1125]
["安徽马钢表面技术股份有限公司","废水排口","化学需氧量(COD)",154.8,"2021-03-07 05:00:00","2021-03-07 08:00:00","0~80",0.935]
["安徽马钢表面技术股份有限公司","废水排口","化学需氧量(COD)",80.588,"2021-03-24 12:00:00","2021-03-24 13:00:00","0~80",0.0074]
["安徽马钢表面技术股份有限公司","废水排口","化学需氧量(COD)",90.011,"2021-03-31 16:00:00","2021-03-31 19:00:00","0~80",0.1251]
["安徽马钢表面技术股份有限公司","超音速废水处理","PH值",5.973,"2021-03-30 14:00:00","2021-03-30 15:00:00","6~9",1.027]
["安徽马钢表面技术股份有限公司","超音速废水处理","化学需氧量(COD)",94.728,"2021-03-05 11:00:00","2021-03-05 12:00:00","0~80",0.1841]
["安徽马钢表面技术股份有限公司","超音速废水处理","化学需氧量(COD)",120.011,"2021-03-19 11:00:00","2021-03-19 13:00:00","0~80",0.5001]
["安徽马钢化工能源科技有限公司","化工能源南东排口","PH值",9.082,"2021-03-02 07:00:00","2021-03-02 08:00:00","6~9",1.041]
["山鹰国际控股股份公司","总排口","化学需氧量(COD)",232.708,"2021-03-01 12:00:00","2021-03-01 14:00:00","0~90",1.5856]
["山鹰国际控股股份公司","总排口","化学需氧量(COD)",187.811,"2021-03-18 16:00:00","2021-03-18 17:00:00","0~90",1.0868]
["山鹰国际控股股份公司","总排口","化学需氧量(COD)",183.997,"2021-03-24 12:00:00","2021-03-24 14:00:00","0~90",1.0444]
["山鹰国际控股股份公司","总排口","总氮",624.639,"2021-03-21 17:00:00","2021-03-21 20:00:00","0~12",51.0533]
["山鹰国际控股股份公司","总排口","总氮",27.628,"2021-03-29 01:00:00","2021-03-29 03:00:00","0~12",1.3023]
["国水（马鞍山）污水处理有限公司","总排","化学需氧量(COD)",75.346,"2021-03-01 11:00:00","2021-03-01 12:00:00","0~60",0.2558]
["马鞍山中铁水务有限公司","总排","化学需氧量(COD)",60.303,"2021-03-01 10:00:00","2021-03-01 12:00:00","0~60",0.0051]
["马鞍山江东中铁水务有限公司","污水出口","化学需氧量(COD)",96.621,"2021-03-03 11:00:00","2021-03-03 12:00:00","0~50",0.9324]
["马鞍山江东中铁水务有限公司","污水出口","化学需氧量(COD)",99.503,"2021-03-08 11:00:00","2021-03-08 13:00:00","0~50",0.9901]
["马鞍山江东中铁水务有限公司","污水出口","总氮",17.219,"2021-03-03 12:00:00","2021-03-03 13:00:00","0~15",0.1479]
["马鞍山江东中铁水务有限公司","污水出口","总氮",20.181,"2021-03-08 11:00:00","2021-03-08 12:00:00","0~15",0.3454]
["马鞍山江东中铁水务有限公司","污水出口","总氮",15.618,"2021-03-19 21:00:00","2021-03-19 22:00:00","0~15",0.0412]
["马鞍山江东中铁水务有限公司","污水出口","总氮",16.167,"2021-03-21 16:00:00","2021-03-21 17:00:00","0~15",0.0778]
["马鞍山江东中铁水务有限公司","污水出口","总磷",1.53,"2021-03-03 12:00:00","2021-03-03 13:00:00","0~1",0.53]
["马鞍山江东中铁水务有限公司","污水出口","总磷",1.918,"2021-03-08 11:00:00","2021-03-08 12:00:00","0~1",0.918]
["马鞍山江东中铁水务有限公司","污水出口","总磷",1.992,"2021-03-31 16:00:00","2021-03-31 17:00:00","0~1",0.992]
["马鞍山钢铁股份有限公司","炼焦南废水西排口","氨氮",17.41,"2021-03-20 05:00:00","2021-03-20 07:00:00","0~10",0.741,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南烧结废水排口","化学需氧量(COD)",56,"2021-03-24 03:00:00","2021-03-24 04:00:00","0~50",0.12,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南烧结废水排口","化学需氧量(COD)",53.216,"2021-03-25 07:00:00","2021-03-25 09:00:00","0~50",0.0643,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南烧结废水排口","化学需氧量(COD)",159.7,"2021-03-28 21:00:00","2021-03-28 23:00:00","0~50",2.194,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","能控北2#排涝泵站","氨氮",5.396,"2021-03-04 07:00:00","2021-03-04 09:00:00","0~5",0.0792,"水质波动"]
["马鞍山钢铁股份有限公司","能控北2#排涝泵站","氨氮",5.04,"2021-03-04 12:00:00","2021-03-04 13:00:00","0~5",0.008,"水质波动"]
["马鞍山钢铁股份有限公司","能控北2#排涝泵站","氨氮",5.156,"2021-03-10 12:00:00","2021-03-10 13:00:00","0~5",0.0312,"仪表比对"]
["马鞍山钢铁股份有限公司","能控北2#排涝泵站","氨氮",7.447,"2021-03-17 13:00:00","2021-03-17 14:00:00","0~5",0.4894,"仪表比对"]
["马鞍山钢铁股份有限公司","能控北2#排涝泵站","氨氮",7.669,"2021-03-24 11:00:00","2021-03-24 12:00:00","0~5",0.5338,"水质波动"]
["马鞍山钢铁股份有限公司","能控北2#排涝泵站","氨氮",9.468,"2021-03-31 11:00:00","2021-03-31 12:00:00","0~5",0.8936,"仪表比对"]
["马鞍山钢铁股份有限公司","能控北3#排涝泵站","PH值",5.63,"2021-03-27 09:00:00","2021-03-27 11:00:00","6~9",1.37,"PH值设备故障"]
["马鞍山钢铁股份有限公司","能控北3#排涝泵站","化学需氧量(COD)",159.9,"2021-03-20 06:00:00","2021-03-20 17:00:00","0~50",2.198,"COD设备电磁阀损坏"]
["马鞍山钢铁股份有限公司","能控北4#排涝泵站","PH值",9.06,"2021-03-20 16:00:00","2021-03-20 17:00:00","6~9",1.03,"水质波动"]
["马鞍山钢铁股份有限公司","能控北4#排涝泵站","化学需氧量(COD)",88.5,"2021-03-04 22:00:00","2021-03-04 23:00:00","0~50",0.77,"水质波动"]
["马鞍山钢铁股份有限公司","能控北4#排涝泵站","化学需氧量(COD)",147.041,"2021-03-08 14:00:00","2021-03-08 15:00:00","0~50",1.9408,"水质波动"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","PH值",9.022,"2021-03-15 18:00:00","2021-03-15 19:00:00","6~9",1.011,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",150.2,"2021-03-01 06:00:00","2021-03-01 07:00:00","0~50",2.004,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",85.7,"2021-03-02 04:00:00","2021-03-02 06:00:00","0~50",0.714,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",61.964,"2021-03-02 20:00:00","2021-03-02 21:00:00","0~50",0.2393,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",140.9,"2021-03-03 04:00:00","2021-03-03 06:00:00","0~50",1.818,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",89.7,"2021-03-07 04:00:00","2021-03-07 06:00:00","0~50",0.794,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",150.248,"2021-03-07 08:00:00","2021-03-07 10:00:00","0~50",2.005,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",171.697,"2021-03-07 12:00:00","2021-03-07 14:00:00","0~50",2.4339,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",172.3,"2021-03-07 18:00:00","2021-03-07 20:00:00","0~50",2.446,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",186.5,"2021-03-08 20:00:00","2021-03-08 21:00:00","0~50",2.73,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",129.3,"2021-03-09 08:00:00","2021-03-09 10:00:00","0~50",1.586,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",54.7,"2021-03-10 04:00:00","2021-03-10 05:00:00","0~50",0.094,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",181.7,"2021-03-11 08:00:00","2021-03-11 10:00:00","0~50",2.634,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",177,"2021-03-11 12:00:00","2021-03-11 14:00:00","0~50",2.54,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",173.195,"2021-03-15 14:00:00","2021-03-15 15:00:00","0~50",2.4639,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",145.437,"2021-03-15 20:00:00","2021-03-16 00:00:00","0~50",1.9087,"大雨导致污水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",83.7,"2021-03-16 06:00:00","2021-03-16 17:00:00","0~50",0.674,"道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",167.1,"2021-03-19 04:00:00","2021-03-19 06:00:00","0~50",2.342,"道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",88,"2021-03-19 08:00:00","2021-03-19 10:00:00","0~50",0.76,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",130.6,"2021-03-20 02:00:00","2021-03-20 06:00:00","0~50",1.612,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",124.2,"2021-03-21 04:00:00","2021-03-21 06:00:00","0~50",1.484,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",144.3,"2021-03-21 14:00:00","2021-03-21 16:00:00","0~50",1.886,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",89.55,"2021-03-24 18:00:00","2021-03-24 19:00:00","0~50",0.791,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",161.7,"2021-03-26 14:00:00","2021-03-26 16:00:00","0~50",2.234,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",185.536,"2021-03-27 06:00:00","2021-03-27 09:00:00","0~50",2.7107,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",65,"2021-03-27 18:00:00","2021-03-27 20:00:00","0~50",0.3,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼铁南铁区废水东排口","化学需氧量(COD)",143.5,"2021-03-30 16:00:00","2021-03-30 18:00:00","0~50",1.87,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","能控南六汾河总排","总氮",15007.211,"2021-03-01 21:00:00","2021-03-01 22:00:00","0~15",999.4807,"设备故障"]
["马鞍山钢铁股份有限公司","能控南六汾河总排","总氮",7507.621,"2021-03-02 14:00:00","2021-03-02 15:00:00","0~15",499.5081,"设备故障"]
["马鞍山钢铁股份有限公司","能控南六汾河总排","总氮",17.359,"2021-03-09 07:00:00","2021-03-09 19:00:00","0~15",0.1573,"设备故障"]
["马鞍山钢铁股份有限公司","炼焦南焦化灰渣废水排口","化学需氧量(COD)",154.554,"2021-03-19 06:00:00","2021-03-19 07:00:00","0~80",0.9319,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼焦南焦化灰渣废水排口","氨氮",10.007,"2021-03-20 23:00:00","2021-03-21 00:00:00","0~10",0.0007,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","炼焦南焦化灰渣废水排口","氨氮",10.103,"2021-03-22 17:00:00","2021-03-22 18:00:00","0~10",0.0103,"下雨道路浑浊积水进入排口，影响检测"]
["马鞍山钢铁股份有限公司","冷轧北水处理排口","化学需氧量(COD)",70.3,"2021-03-08 10:00:00","2021-03-08 11:00:00","0~70",0.0043,"安徽省计量院量值溯源"]
["马鞍山钢铁股份有限公司","冷轧北水处理排口","化学需氧量(COD)",72.8,"2021-03-12 10:00:00","2021-03-12 11:00:00","0~70",0.04,"安徽省计量院量值溯源"]
["马鞍山钢铁股份有限公司","特钢废水总排","PH值",9.011,"2021-03-03 06:00:00","2021-03-03 08:00:00","6~9",1.0055,"下雨排口水量变化，PH调节致短时超标"]
["马鞍山钢铁股份有限公司","特钢废水总排","PH值",5.173,"2021-03-04 09:00:00","2021-03-04 10:00:00","6~9",1.827,"下雨排口水量变化，PH调节致短时超标"]
["马鞍山钢铁股份有限公司","特钢废水总排","PH值",5.93,"2021-03-04 12:00:00","2021-03-04 13:00:00","6~9",1.07,"下雨排口水量变化，PH调节致短时超标"]
["马鞍山钢铁股份有限公司","特钢废水总排","PH值",9.066,"2021-03-07 03:00:00","2021-03-07 05:00:00","6~9",1.033,"下雨排口水量变化，PH调节致短时超标"]
["马鞍山钢铁股份有限公司","特钢废水总排","PH值",5.36,"2021-03-07 06:00:00","2021-03-07 07:00:00","6~9",1.64,"下雨排口水量变化，PH调节致短时超标"]
["马鞍山钢铁股份有限公司","轮轴废水排口","PH值",9.062,"2021-03-19 17:00:00","2021-03-19 18:00:00","6~9",1.031]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",58.7,"2021-03-19 18:00:00","2021-03-19 19:00:00","0~50",0.174]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",68.4,"2021-03-20 20:00:00","2021-03-20 21:00:00","0~50",0.368]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",50.583,"2021-03-22 14:00:00","2021-03-22 15:00:00","0~50",0.0117]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",63.3,"2021-03-22 18:00:00","2021-03-22 20:00:00","0~50",0.266]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",60.37,"2021-03-24 07:00:00","2021-03-24 09:00:00","0~50",0.2074]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",60.9,"2021-03-24 12:00:00","2021-03-24 14:00:00","0~50",0.218]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",50.3,"2021-03-24 20:00:00","2021-03-24 21:00:00","0~50",0.006]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",50.6,"2021-03-27 14:00:00","2021-03-27 15:00:00","0~50",0.012]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",64.7,"2021-03-29 12:00:00","2021-03-29 14:00:00","0~50",0.294]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",53.8,"2021-03-29 18:00:00","2021-03-30 00:00:00","0~50",0.076]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",59.3,"2021-03-30 20:00:00","2021-03-30 21:00:00","0~50",0.186]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",60.5,"2021-03-31 08:00:00","2021-03-31 10:00:00","0~50",0.21]
["马鞍山钢铁股份有限公司","轮轴废水排口","化学需氧量(COD)",96.3,"2021-03-31 18:00:00","2021-03-31 19:00:00","0~50",0.926]
["马鞍山钢铁股份有限公司","长材北废水总排排口","PH值",0,"2021-03-22 15:00:00","2021-03-22 16:00:00","6~9",7,"数采仪掉线，期间PH值无数据"]
["马鞍山钢铁股份有限公司","能控北292废水排口","PH值",11.492,"2021-03-22 05:00:00","2021-03-22 06:00:00","6~9",2.246,"PH探头故障"]
["马鞍山钢铁股份有限公司","能控北292废水排口","PH值",9.325,"2021-03-30 09:00:00","2021-03-30 10:00:00","6~9",1.1625,"水质波动"]
["马鞍山钢铁股份有限公司","热电北废水排口","PH值",9.418,"2021-03-20 13:00:00","2021-03-20 14:00:00","6~9",1.209,"水质波动"]
["光大江东环保能源（马鞍山）有限公司","3#炉","一氧化碳",116.066,"2021-03-01 00:00:00","2021-03-13 20:00:00","0~60",0.9344]
["光大江东环保能源（马鞍山）有限公司","3#炉","氮氧化物",488.617,"2021-03-01 00:00:00","2021-03-13 20:00:00","0~300",0.6287]
["光大江东环保能源（马鞍山）有限公司","3#炉","氯化氢",65.017,"2021-03-01 09:00:00","2021-03-13 20:00:00","0~60",0.0836]
["马鞍山钢铁股份有限公司","炼铁南2#烧结机排口","氮氧化物",374.7,"2021-03-01 16:00:00","2021-03-01 17:00:00","0~300",0.249,"仪表标定"]
["马鞍山澳新环保科技有限公司","焚烧炉","一氧化碳",127.264,"2021-03-02 06:00:00","2021-03-02 07:00:00","0~80",0.5908,"仪表标定"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.6,"2021-03-03 17:00:00","2021-03-03 18:00:00","0~30",0.02,"仪表标定"]
["马鞍山澳新环保科技有限公司","焚烧炉","一氧化碳",120.324,"2021-03-04 06:00:00","2021-03-04 07:00:00","0~80",0.5041]
["马鞍山钢铁股份有限公司","炼焦南5#6#焦炉出焦除尘","二氧化硫",38.98,"2021-03-04 10:00:00","2021-03-04 11:00:00","0~30",0.2993,"仪表标定"]
["国能神皖马鞍山发电有限责任公司","4号机组废气排放口","烟尘",65.209,"2021-03-04 21:00:00","2021-03-29 11:00:00","0~20",2.2605]
["马鞍山钢铁股份有限公司","炼铁南1#烧结机机低硫段","二氧化硫",189.92,"2021-03-05 10:00:00","2021-03-05 11:00:00","0~180",0.0551,"仪表标定"]
["马鞍山石溪野水泥有限责任公司","2#磨排口","烟尘",10.4,"2021-03-05 14:00:00","2021-03-05 15:00:00","0~10",0.04]
["马鞍山澳新环保科技有限公司","焚烧炉","一氧化碳",82.412,"2021-03-07 05:00:00","2021-03-07 06:00:00","0~80",0.0302]
["马鞍山钢铁股份有限公司","炼焦南2#焦炉排口","二氧化硫",30.411,"2021-03-07 17:00:00","2021-03-07 18:00:00","0~30",0.0137,"检测设备故障"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",32.43,"2021-03-09 09:00:00","2021-03-09 10:00:00","0~30",0.081,"仪表故障"]
["马鞍山钢铁股份有限公司","炼焦南2#焦炉排口","烟尘",16.279,"2021-03-08 18:00:00","2021-03-08 19:00:00","0~15",0.0853,"CEMS采样管积水"]
["马鞍山钢铁股份有限公司","炼铁南4#炉槽下除尘","烟尘",10.1,"2021-03-10 10:00:00","2021-03-10 11:00:00","0~10",0.01,"仪表标定"]
["马鞍山钢铁股份有限公司","炼铁南2#炉炉前除尘","烟尘",20.3,"2021-03-12 11:00:00","2021-03-12 12:00:00","0~15",0.3533,"仪表标定"]
["马鞍山钢铁股份有限公司","炼铁南2#烧结机排口","烟尘",75.7,"2021-03-12 17:00:00","2021-03-12 20:00:00","0~40",0.8925,"脱硫雾化器故障"]
["马鞍山钢铁股份有限公司","炼铁南3#竖炉脱硫排口","二氧化硫",280.59,"2021-03-13 00:00:00","2021-03-13 01:00:00","0~180",0.5588,"检修启停机"]
["马鞍山钢铁股份有限公司","炼铁南2#烧结机排口","二氧化硫",194.36,"2021-03-13 00:00:00","2021-03-13 01:00:00","0~180",0.0798,"启停机"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",31.28,"2021-03-14 22:00:00","2021-03-14 23:00:00","0~30",0.0427,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南3#4#焦炉排口","烟尘",16.54,"2021-03-15 17:00:00","2021-03-15 18:00:00","0~15",0.1027,"焦炉炉墙串漏，导致烟尘超标"]
["马鞍山钢铁股份有限公司","炼焦南3#4#焦炉排口","烟尘",16.67,"2021-03-15 21:00:00","2021-03-15 22:00:00","0~15",0.1113,"焦炉炉墙串漏，导致烟尘超标"]
["马鞍山钢铁股份有限公司","炼焦北4#干熄焦放散气脱硫","二氧化硫",93.843,"2021-03-16 20:00:00","2021-03-16 21:00:00","0~80",0.173,"给料振动电机脱落，无法下料，短时超标"]
["马鞍山钢铁股份有限公司","炼焦北5#干熄焦放散气脱硫","二氧化硫",97.184,"2021-03-16 21:00:00","2021-03-16 22:00:00","0~80",0.2148,"给料振动电机脱落，无法下料，短时超标"]
["马鞍山钢铁股份有限公司","热电北12#炉脱硫排口","烟尘",18.58,"2021-03-17 07:00:00","2021-03-29 09:00:00","0~5",2.716,"停炉检修"]
["马鞍山澳新环保科技有限公司","焚烧炉","一氧化碳",922.37,"2021-03-06 03:00:00","2021-03-06 06:00:00","0~80",10.5296]
["马鞍山澳新环保科技有限公司","焚烧炉","烟尘",86.631,"2021-03-06 03:00:00","2021-03-06 05:00:00","0~80",0.0829]
["马鞍山钢铁股份有限公司","炼焦北4#5#干熄焦除尘","二氧化硫",128.58,"2021-03-16 21:00:00","2021-03-16 23:00:00","0~80",0.6073,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼铁南3#烧结机排口","二氧化硫",184.36,"2021-03-21 21:00:00","2021-03-21 22:00:00","0~180",0.0242,"煤气压力低，3#脱硫热风炉熄火"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.18,"2021-03-22 21:00:00","2021-03-22 22:00:00","0~30",0.006,"仪表标定"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",46.59,"2021-03-23 11:00:00","2021-03-23 12:00:00","0~30",0.553,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南3#干熄焦放散气脱硫","二氧化硫",173.121,"2021-03-23 22:00:00","2021-03-24 01:00:00","0~80",1.164,"生产工艺调整"]
["山鹰国际控股股份公司","2号脱硫塔","二氧化硫",88.145,"2021-03-25 09:00:00","2021-03-25 10:00:00","0~50",0.7629]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",31.3,"2021-03-25 10:00:00","2021-03-25 11:00:00","0~30",0.0433,"硫化风机故障"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",49.06,"2021-03-18 05:00:00","2021-03-18 07:00:00","0~30",0.6353,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼铁南2#烧结机排口","氮氧化物",344.3,"2021-03-22 10:00:00","2021-03-22 11:00:00","0~300",0.1477,"仪表标定"]
["光大江东环保能源（马鞍山）有限公司","3#炉","氯化氢",64.725,"2021-03-25 14:00:00","2021-03-25 15:00:00","0~60",0.0788]
["马鞍山钢铁股份有限公司","炼焦南1、2#干熄焦放散气脱硫","二氧化硫",92.249,"2021-03-25 16:00:00","2021-03-25 17:00:00","0~80",0.1531,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼铁南1#烧结机机尾除尘","烟尘",24.45,"2021-03-25 21:00:00","2021-03-25 22:00:00","0~20",0.2225,"一电场轻微故障"]
["安徽马钢嘉华新型建材有限公司","2#线","烟尘",21,"2021-03-26 12:00:00","2021-03-26 13:00:00","0~20",0.05]
["山鹰国际控股股份公司","6号炉","氮氧化物",195.894,"2021-03-26 14:00:00","2021-03-26 19:00:00","0~100",0.9589]
["马鞍山钢铁股份有限公司","热电南5#炉排口","二氧化硫",36.256,"2021-03-26 16:00:00","2021-03-26 17:00:00","0~35",0.0359,"因煤气品质差，导致烟尘短时超标"]
["山鹰国际控股股份公司","8号炉","烟尘",12.299,"2021-03-27 04:00:00","2021-03-27 05:00:00","0~10",0.2299]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.35,"2021-03-27 06:00:00","2021-03-27 07:00:00","0~30",0.0117,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",30.76,"2021-03-28 04:00:00","2021-03-28 05:00:00","0~30",0.0253,"斜槽下料不均匀，硫化风机堵塞。"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.14,"2021-03-28 20:00:00","2021-03-28 21:00:00","0~30",0.0047,"生产工艺调整"]
["山鹰国际控股股份公司","1号脱硫塔","二氧化硫",80.252,"2021-03-29 15:00:00","2021-03-29 16:00:00","0~50",0.605]
["山鹰国际控股股份公司","9号炉","氮氧化物",113.625,"2021-03-02 09:00:00","2021-03-02 11:00:00","0~50",1.2725]
["马鞍山钢铁股份有限公司","炼焦南3#4#焦炉出焦除尘","二氧化硫",58.59,"2021-03-10 10:00:00","2021-03-10 11:00:00","0~30",0.953,"仪表标定"]
["马鞍山钢铁股份有限公司","热电北12#炉脱硫排口","二氧化硫",35.19,"2021-03-17 04:00:00","2021-03-17 05:00:00","0~35",0.0054,"停炉"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.69,"2021-03-25 00:00:00","2021-03-25 01:00:00","0~30",0.023,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",34.89,"2021-03-25 07:00:00","2021-03-25 09:00:00","0~30",0.163,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",31.15,"2021-03-27 05:00:00","2021-03-27 06:00:00","0~30",0.0383,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",33.12,"2021-03-30 15:00:00","2021-03-30 16:00:00","0~30",0.104,"生产工艺调整"]
["光大江东环保能源（马鞍山）有限公司","1#炉","氯化氢",84.968,"2021-03-31 11:00:00","2021-03-31 12:00:00","0~60",0.4161]
["马鞍山钢铁股份有限公司","炼焦北4#5#干熄焦除尘","二氧化硫",86.25,"2021-03-31 19:00:00","2021-03-31 20:00:00","0~80",0.0781,"停机检修"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",34.3,"2021-03-31 22:00:00","2021-04-01 00:00:00","0~30",0.1433,"停机检修"]
["马鞍山钢铁股份有限公司","炼焦南1#焦炉排口","二氧化硫",62.38,"2021-03-17 09:00:00","2021-03-17 10:00:00","0~30",1.0793,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南2#焦炉排口","二氧化硫",37.901,"2021-03-17 08:00:00","2021-03-17 09:00:00","0~30",0.2634,"生产工艺调整"]
["安徽马钢嘉华新型建材有限公司","2#线","烟尘",24.3,"2021-03-19 15:00:00","2021-03-19 16:00:00","0~20",0.215]
["马鞍山钢铁股份有限公司","炼焦南3#干熄焦环境除尘","二氧化硫",92.2338,"2021-03-21 12:00:00","2021-03-21 13:00:00","0~80",0.1529,"检修布袋，导致间隙超标"]
["马鞍山澳新环保科技有限公司","焚烧炉","一氧化碳",118.951,"2021-03-21 21:00:00","2021-03-21 22:00:00","0~80",0.4869]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.71,"2021-03-25 20:00:00","2021-03-25 21:00:00","0~30",0.0237,"生产工艺调整"]
["山鹰国际控股股份公司","9号炉","氮氧化物",82.31,"2021-03-03 09:00:00","2021-03-03 11:00:00","0~50",0.6462]
["马鞍山钢铁股份有限公司","炼焦南3#干熄焦放散气脱硫","二氧化硫",141.479,"2021-03-16 05:00:00","2021-03-16 06:00:00","0~80",0.7685,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",40.29,"2021-03-18 01:00:00","2021-03-18 03:00:00","0~30",0.343,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.36,"2021-03-28 02:00:00","2021-03-28 03:00:00","0~30",0.012,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",41.87,"2021-03-31 19:00:00","2021-03-31 21:00:00","0~30",0.3957,"停机检修"]
["马鞍山钢铁股份有限公司","炼铁南3#竖炉脱硫排口","二氧化硫",223.43,"2021-03-10 20:00:00","2021-03-10 21:00:00","0~180",0.2413,"产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南1、2#干熄焦放散气脱硫","二氧化硫",453.002,"2021-03-20 03:00:00","2021-03-20 06:00:00","0~80",4.6625,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.68,"2021-03-20 05:00:00","2021-03-20 06:00:00","0~30",0.0227,"生产工艺调整"]
["山鹰国际控股股份公司","1号脱硫塔","二氧化硫",80.689,"2021-03-26 07:00:00","2021-03-26 10:00:00","0~50",0.6138,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",30.22,"2021-03-17 19:00:00","2021-03-17 20:00:00","0~30",0.0073,"生产工艺调整"]
["皖能马鞍山发电有限公司","2号机组废气排口","烟尘",55.68,"2021-03-18 21:00:00","/","0~20",1.784,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦南3#4#焦炉排口","氮氧化物",150.16,"2021-03-23 05:00:00","2021-03-23 06:00:00","0~150",0.0011,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",30.53,"2021-03-24 08:00:00","2021-03-24 09:00:00","0~30",0.0177,"生产工艺调整"]
["马鞍山钢铁股份有限公司","炼焦北8#焦炉脱硫脱硝排口","二氧化硫",32.01,"2021-03-24 09:00:00","2021-03-24 10:00:00","0~30",0.067,"仪表标定"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",45.22,"2021-03-24 10:00:00","2021-03-24 11:00:00","0~30",0.5073,"仪表标定"]
["马鞍山钢铁股份有限公司","炼铁南2#炉顶吸除尘","烟尘",15.74,"2021-03-26 10:00:00","2021-03-26 11:00:00","0~15",0.0493,"仪表标定"]
["马鞍山钢铁股份有限公司","炼铁南1#烧结机机尾除尘","烟尘",23.27,"2021-03-22 21:00:00","2021-03-22 22:00:00","0~20",0.1635,"生产工艺调整"]
["山鹰国际控股股份公司","6号炉","二氧化硫",69.282,"2021-03-26 16:00:00","2021-03-26 18:00:00","0~50",0.3856]
["马鞍山钢铁股份有限公司","热电南5#炉排口","二氧化硫",37.242,"2021-03-29 13:00:00","2021-03-29 15:00:00","0~35",0.0641,"因煤气品质差，导致烟尘短时超标"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",31.77,"2021-03-28 09:00:00","2021-03-28 13:00:00","0~30",0.059,"停机检修"]
["马鞍山钢铁股份有限公司","炼焦南5#焦炉排口","二氧化硫",72.67,"2021-03-31 15:00:00","2021-03-31 16:00:00","0~30",1.4223,"停机检修"]
["马鞍山钢铁股份有限公司","炼焦北7#8#焦炉出焦除尘","二氧化硫",33.35,"2021-03-31 15:00:00","2021-03-31 16:00:00","0~30",0.1117,"仪表标定"]
["马鞍山钢铁股份有限公司","炼铁南1#2#竖炉脱硫排口","氮氧化物",354.78,"2021-03-30 09:00:00","2021-03-30 10:00:00","0~300",0.1826,"仪表标定"]
["马鞍山澳新环保科技有限公司","焚烧炉","一氧化碳",84.792,"2021-03-30 18:00:00","2021-03-30 19:00:00","0~80",0.0599]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}